### Setup Failed

Check the following items, and then perform network setup again.
Check that the access point (wireless router) is turned on. If it is turned on, turn the access point’s (wireless router’s) power off and on again. Consider other users who may be using the network.
Disable the privacy separator on the access point (wireless router).
Place your printer close to the access point (wireless router).
Check that the access point (wireless router) supports WPS. If it does not support WPS, you cannot establish a network using Push Button Setup (WPS).
If the MAC address filtering function is enabled, register your printer’s MAC address to prevent your printer from being filtered. See the documentation provided with the access point for registering.
Check that the Wi-Fi communication mode (IEEE802.11*) set for your access point (wireless router) matches the one supported by your printer. (*Display varies according to your location.)